(kicad_sch
	(version 20231120)
	(generator "eeschema")
	(generator_version "8.0")
	(paper "A4")
	(title_block
		(title "Voltmetr s ADS1115")
		(company "Jirka Chráska")
	)
	(lib_symbols
		(symbol "Analog_ADC:ADS1115IDGS"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 2.54 13.97 0)
			)
			(property "Value" "ADS1115IDGS"
				(at 7.62 11.43 0)
			)
			(property "Footprint" "Package_SO:TSSOP-10_3x3mm_P0.5mm"
				(at 0 -12.7 0)
			)
			(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads1113.pdf"
				(at -1.27 -22.86 0)
			)
			(property "Description" "Ultra-Small, Low-Power, I2C-Compatible, 860-SPS, 16-Bit ADCs With Internal Reference, Oscillator, and Programmable Comparator, VSSOP-10"
				(at 0 0 0)
			)
			(property "ki_keywords" "16 bit 4 channel I2C ADC"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "TSSOP*3x3mm*P0.5mm*"
				(at 0 0 0)
			)
			(symbol "ADS1115IDGS_0_1"
				(rectangle
					(start -7.62 10.16)
					(end 7.62 -7.62)
					(fill
						(type background)
					)
				)
			)
			(symbol "ADS1115IDGS_1_1"
				(pin input line
					(at 10.16 -5.08 180)
					(length 2.54)
					(name "ADDR")
					(number "1")
				)
				(pin input line
					(at 10.16 0 180)
					(length 2.54)
					(name "SCL")
					(number "10")
				)
				(pin output line
					(at 10.16 5.08 180)
					(length 2.54)
					(name "ALERT/RDY")
					(number "2")
				)
				(pin power_in line
					(at 0 -10.16 90)
					(length 2.54)
					(name "GND")
					(number "3")
				)
				(pin input line
					(at -10.16 2.54 0)
					(length 2.54)
					(name "AIN0")
					(number "4")
				)
				(pin input line
					(at -10.16 0 0)
					(length 2.54)
					(name "AIN1")
					(number "5")
				)
				(pin input line
					(at -10.16 -2.54 0)
					(length 2.54)
					(name "AIN2")
					(number "6")
				)
				(pin input line
					(at -10.16 -5.08 0)
					(length 2.54)
					(name "AIN3")
					(number "7")
				)
				(pin power_in line
					(at 0 12.7 270)
					(length 2.54)
					(name "VDD")
					(number "8")
				)
				(pin bidirectional line
					(at 10.16 -2.54 180)
					(length 2.54)
					(name "SDA")
					(number "9")
				)
			)
		)
		(symbol "Device:R"
			(pin_numbers hide)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R"
				(at 0 0 90)
			)
			(property "Footprint" ""
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "Device:R_Potentiometer"
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "RV"
				(at -4.445 0 90)
			)
			(property "Value" "R_Potentiometer"
				(at -2.54 0 90)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Potentiometer"
				(at 0 0 0)
			)
			(property "ki_keywords" "resistor variable"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Potentiometer*"
				(at 0 0 0)
			)
			(symbol "R_Potentiometer_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 1.524 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.143 0) (xy 2.286 0.508) (xy 2.286 -0.508) (xy 1.143 0)
					)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 1.016 2.54)
					(end -1.016 -2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_Potentiometer_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 1.27)
					(name "2")
					(number "2")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "3")
					(number "3")
				)
			)
		)
		(symbol "MCU_RaspberryPi_and_Boards:Pico"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -13.97 27.94 0)
			)
			(property "Value" "Pico"
				(at 0 19.05 0)
			)
			(property "Footprint" "RPi_Pico:RPi_Pico_SMD_TH"
				(at 0 0 90)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(symbol "Pico_0_0"
				(text "Raspberry Pi Pico"
					(at 0 21.59 0)
				)
			)
			(symbol "Pico_0_1"
				(rectangle
					(start -15.24 26.67)
					(end 15.24 -26.67)
					(fill
						(type background)
					)
				)
			)
			(symbol "Pico_1_1"
				(pin bidirectional line
					(at -17.78 24.13 0)
					(length 2.54)
					(name "GPIO0")
					(number "1")
				)
				(pin bidirectional line
					(at -17.78 1.27 0)
					(length 2.54)
					(name "GPIO7")
					(number "10")
				)
				(pin bidirectional line
					(at -17.78 -1.27 0)
					(length 2.54)
					(name "GPIO8")
					(number "11")
				)
				(pin bidirectional line
					(at -17.78 -3.81 0)
					(length 2.54)
					(name "GPIO9")
					(number "12")
				)
				(pin power_in line
					(at -17.78 -6.35 0)
					(length 2.54)
					(name "GND")
					(number "13")
				)
				(pin bidirectional line
					(at -17.78 -8.89 0)
					(length 2.54)
					(name "GPIO10")
					(number "14")
				)
				(pin bidirectional line
					(at -17.78 -11.43 0)
					(length 2.54)
					(name "GPIO11")
					(number "15")
				)
				(pin bidirectional line
					(at -17.78 -13.97 0)
					(length 2.54)
					(name "GPIO12")
					(number "16")
				)
				(pin bidirectional line
					(at -17.78 -16.51 0)
					(length 2.54)
					(name "GPIO13")
					(number "17")
				)
				(pin power_in line
					(at -17.78 -19.05 0)
					(length 2.54)
					(name "GND")
					(number "18")
				)
				(pin bidirectional line
					(at -17.78 -21.59 0)
					(length 2.54)
					(name "GPIO14")
					(number "19")
				)
				(pin bidirectional line
					(at -17.78 21.59 0)
					(length 2.54)
					(name "GPIO1")
					(number "2")
				)
				(pin bidirectional line
					(at -17.78 -24.13 0)
					(length 2.54)
					(name "GPIO15")
					(number "20")
				)
				(pin bidirectional line
					(at 17.78 -24.13 180)
					(length 2.54)
					(name "GPIO16")
					(number "21")
				)
				(pin bidirectional line
					(at 17.78 -21.59 180)
					(length 2.54)
					(name "GPIO17")
					(number "22")
				)
				(pin power_in line
					(at 17.78 -19.05 180)
					(length 2.54)
					(name "GND")
					(number "23")
				)
				(pin bidirectional line
					(at 17.78 -16.51 180)
					(length 2.54)
					(name "GPIO18")
					(number "24")
				)
				(pin bidirectional line
					(at 17.78 -13.97 180)
					(length 2.54)
					(name "GPIO19")
					(number "25")
				)
				(pin bidirectional line
					(at 17.78 -11.43 180)
					(length 2.54)
					(name "GPIO20")
					(number "26")
				)
				(pin bidirectional line
					(at 17.78 -8.89 180)
					(length 2.54)
					(name "GPIO21")
					(number "27")
				)
				(pin power_in line
					(at 17.78 -6.35 180)
					(length 2.54)
					(name "GND")
					(number "28")
				)
				(pin bidirectional line
					(at 17.78 -3.81 180)
					(length 2.54)
					(name "GPIO22")
					(number "29")
				)
				(pin power_in line
					(at -17.78 19.05 0)
					(length 2.54)
					(name "GND")
					(number "3")
				)
				(pin input line
					(at 17.78 -1.27 180)
					(length 2.54)
					(name "RUN")
					(number "30")
				)
				(pin bidirectional line
					(at 17.78 1.27 180)
					(length 2.54)
					(name "GPIO26_ADC0")
					(number "31")
				)
				(pin bidirectional line
					(at 17.78 3.81 180)
					(length 2.54)
					(name "GPIO27_ADC1")
					(number "32")
				)
				(pin power_in line
					(at 17.78 6.35 180)
					(length 2.54)
					(name "AGND")
					(number "33")
				)
				(pin bidirectional line
					(at 17.78 8.89 180)
					(length 2.54)
					(name "GPIO28_ADC2")
					(number "34")
				)
				(pin power_in line
					(at 17.78 11.43 180)
					(length 2.54)
					(name "ADC_VREF")
					(number "35")
				)
				(pin power_in line
					(at 17.78 13.97 180)
					(length 2.54)
					(name "3V3")
					(number "36")
				)
				(pin input line
					(at 17.78 16.51 180)
					(length 2.54)
					(name "3V3_EN")
					(number "37")
				)
				(pin bidirectional line
					(at 17.78 19.05 180)
					(length 2.54)
					(name "GND")
					(number "38")
				)
				(pin power_in line
					(at 17.78 21.59 180)
					(length 2.54)
					(name "VSYS")
					(number "39")
				)
				(pin bidirectional line
					(at -17.78 16.51 0)
					(length 2.54)
					(name "GPIO2")
					(number "4")
				)
				(pin power_in line
					(at 17.78 24.13 180)
					(length 2.54)
					(name "VBUS")
					(number "40")
				)
				(pin input line
					(at -2.54 -29.21 90)
					(length 2.54)
					(name "SWCLK")
					(number "41")
				)
				(pin power_in line
					(at 0 -29.21 90)
					(length 2.54)
					(name "GND")
					(number "42")
				)
				(pin bidirectional line
					(at 2.54 -29.21 90)
					(length 2.54)
					(name "SWDIO")
					(number "43")
				)
				(pin bidirectional line
					(at -17.78 13.97 0)
					(length 2.54)
					(name "GPIO3")
					(number "5")
				)
				(pin bidirectional line
					(at -17.78 11.43 0)
					(length 2.54)
					(name "GPIO4")
					(number "6")
				)
				(pin bidirectional line
					(at -17.78 8.89 0)
					(length 2.54)
					(name "GPIO5")
					(number "7")
				)
				(pin power_in line
					(at -17.78 6.35 0)
					(length 2.54)
					(name "GND")
					(number "8")
				)
				(pin bidirectional line
					(at -17.78 3.81 0)
					(length 2.54)
					(name "GPIO6")
					(number "9")
				)
			)
		)
		(symbol "OLED_SSD1306:OLED_SSD1306_128x32"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "M"
				(at 0 0 0)
			)
			(property "Value" ""
				(at 0 0 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(symbol "OLED_SSD1306_128x32_0_1"
				(rectangle
					(start 0 -1.27)
					(end 33.02 -13.97)
					(fill
						(type none)
					)
				)
			)
			(symbol "OLED_SSD1306_128x32_1_1"
				(text_box "OLED display SSD1306 132x24 I2c"
					(at 6.35 -2.54 0)
					(size 25.4 -10.16)
					(fill
						(type color)
						(color 0 194 194 1)
					)
				)
				(pin bidirectional line
					(at -2.54 -3.81 0)
					(length 2.54)
					(name "SDA")
					(number "1")
				)
				(pin bidirectional line
					(at -2.54 -6.35 0)
					(length 2.54)
					(name "SCL")
					(number "2")
				)
				(pin power_in line
					(at -2.54 -8.89 0)
					(length 2.54)
					(name "VCC")
					(number "3")
				)
				(pin power_in line
					(at -2.54 -11.43 0)
					(length 2.54)
					(name "GND")
					(number "4")
				)
			)
		)
		(symbol "power:GNDD"
			(power)
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GNDD"
				(at 0 -3.175 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GNDD\" , digital ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "GNDD_0_1"
				(rectangle
					(start -1.27 -1.524)
					(end 1.27 -2.032)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.524)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GNDD_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~")
					(number "1")
				)
			)
		)
	)
	(junction
		(at 104.14 85.09)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 104.14 53.34)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 127 53.34)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 140.97 85.09) (xy 163.83 85.09)
		)
	)
	(wire
		(pts
			(xy 85.09 72.39) (xy 93.98 72.39)
		)
	)
	(wire
		(pts
			(xy 104.14 53.34) (xy 104.14 62.23)
		)
	)
	(wire
		(pts
			(xy 137.16 82.55) (xy 163.83 82.55)
		)
	)
	(wire
		(pts
			(xy 143.51 87.63) (xy 163.83 87.63)
		)
	)
	(wire
		(pts
			(xy 115.57 97.79) (xy 143.51 97.79)
		)
	)
	(wire
		(pts
			(xy 114.3 77.47) (xy 163.83 77.47)
		)
	)
	(wire
		(pts
			(xy 143.51 97.79) (xy 143.51 87.63)
		)
	)
	(wire
		(pts
			(xy 81.28 68.58) (xy 81.28 64.77)
		)
	)
	(wire
		(pts
			(xy 146.05 102.87) (xy 146.05 95.25)
		)
	)
	(wire
		(pts
			(xy 160.02 74.93) (xy 160.02 80.01)
		)
	)
	(wire
		(pts
			(xy 160.02 80.01) (xy 163.83 80.01)
		)
	)
	(wire
		(pts
			(xy 199.39 74.93) (xy 201.93 74.93)
		)
	)
	(wire
		(pts
			(xy 81.28 85.09) (xy 104.14 85.09)
		)
	)
	(wire
		(pts
			(xy 201.93 53.34) (xy 127 53.34)
		)
	)
	(wire
		(pts
			(xy 104.14 85.09) (xy 137.16 85.09)
		)
	)
	(wire
		(pts
			(xy 127 53.34) (xy 104.14 53.34)
		)
	)
	(wire
		(pts
			(xy 81.28 57.15) (xy 81.28 53.34)
		)
	)
	(wire
		(pts
			(xy 115.57 102.87) (xy 146.05 102.87)
		)
	)
	(wire
		(pts
			(xy 81.28 76.2) (xy 81.28 85.09)
		)
	)
	(wire
		(pts
			(xy 137.16 85.09) (xy 137.16 82.55)
		)
	)
	(wire
		(pts
			(xy 114.3 74.93) (xy 160.02 74.93)
		)
	)
	(wire
		(pts
			(xy 115.57 95.25) (xy 140.97 95.25)
		)
	)
	(wire
		(pts
			(xy 201.93 53.34) (xy 201.93 74.93)
		)
	)
	(wire
		(pts
			(xy 115.57 100.33) (xy 127 100.33)
		)
	)
	(wire
		(pts
			(xy 140.97 95.25) (xy 140.97 85.09)
		)
	)
	(wire
		(pts
			(xy 127 100.33) (xy 127 53.34)
		)
	)
	(wire
		(pts
			(xy 146.05 95.25) (xy 163.83 95.25)
		)
	)
	(wire
		(pts
			(xy 81.28 53.34) (xy 104.14 53.34)
		)
	)
	(symbol
		(lib_id "OLED_SSD1306:OLED_SSD1306_128x32")
		(at 113.03 91.44 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "M1"
			(at 78.74 98.4249 0)
		)
		(property "Value" "~"
			(at 78.74 100.33 0)
		)
		(property "Footprint" ""
			(at 113.03 91.44 0)
		)
		(property "Datasheet" ""
			(at 113.03 91.44 0)
		)
		(property "Description" ""
			(at 113.03 91.44 0)
		)
		(pin "3")
		(pin "4")
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "M1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Analog_ADC:ADS1115IDGS")
		(at 104.14 74.93 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U2"
			(at 106.3341 59.69 0)
		)
		(property "Value" "ADS1115IDGS"
			(at 106.3341 62.23 0)
		)
		(property "Footprint" "Package_SO:TSSOP-10_3x3mm_P0.5mm"
			(at 104.14 87.63 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads1113.pdf"
			(at 102.87 97.79 0)
		)
		(property "Description" "Ultra-Small, Low-Power, I2C-Compatible, 860-SPS, 16-Bit ADCs With Internal Reference, Oscillator, and Programmable Comparator, VSSOP-10"
			(at 104.14 74.93 0)
		)
		(pin "1")
		(pin "5")
		(pin "3")
		(pin "4")
		(pin "9")
		(pin "7")
		(pin "8")
		(pin "2")
		(pin "10")
		(pin "6")
		(instances
			(project ""
				(path
					(reference "U2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GNDD")
		(at 104.14 85.09 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01"
			(at 104.14 91.44 0)
		)
		(property "Value" "GND"
			(at 104.14 88.9 0)
		)
		(property "Footprint" ""
			(at 104.14 85.09 0)
		)
		(property "Datasheet" ""
			(at 104.14 85.09 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GNDD\" , digital ground"
			(at 104.14 85.09 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR01")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "MCU_RaspberryPi_and_Boards:Pico")
		(at 181.61 88.9 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U1"
			(at 181.61 57.15 0)
		)
		(property "Value" "Pico"
			(at 181.61 59.69 0)
		)
		(property "Footprint" "RPi_Pico:RPi_Pico_SMD_TH"
			(at 181.61 88.9 90)
		)
		(property "Datasheet" ""
			(at 181.61 88.9 0)
		)
		(property "Description" ""
			(at 181.61 88.9 0)
		)
		(pin "9")
		(pin "8")
		(pin "6")
		(pin "7")
		(pin "33")
		(pin "19")
		(pin "21")
		(pin "20")
		(pin "17")
		(pin "5")
		(pin "30")
		(pin "18")
		(pin "38")
		(pin "42")
		(pin "26")
		(pin "22")
		(pin "10")
		(pin "40")
		(pin "4")
		(pin "16")
		(pin "15")
		(pin "43")
		(pin "31")
		(pin "39")
		(pin "34")
		(pin "41")
		(pin "24")
		(pin "28")
		(pin "13")
		(pin "14")
		(pin "12")
		(pin "2")
		(pin "23")
		(pin "37")
		(pin "36")
		(pin "29")
		(pin "11")
		(pin "3")
		(pin "27")
		(pin "25")
		(pin "32")
		(pin "35")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "U1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 81.28 60.96 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R1"
			(at 83.82 59.6899 0)
		)
		(property "Value" "220"
			(at 83.82 62.2299 0)
		)
		(property "Footprint" ""
			(at 79.502 60.96 90)
		)
		(property "Datasheet" "~"
			(at 81.28 60.96 0)
		)
		(property "Description" "Resistor"
			(at 81.28 60.96 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R_Potentiometer")
		(at 81.28 72.39 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "RV1"
			(at 78.74 71.1199 0)
		)
		(property "Value" "10k"
			(at 78.74 73.6599 0)
		)
		(property "Footprint" ""
			(at 81.28 72.39 0)
		)
		(property "Datasheet" "~"
			(at 81.28 72.39 0)
		)
		(property "Description" "Potentiometer"
			(at 81.28 72.39 0)
		)
		(pin "2")
		(pin "1")
		(pin "3")
		(instances
			(project ""
				(path
					(reference "RV1")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
)
