(kicad_sch
	(version 20231120)
	(generator "eeschema")
	(generator_version "8.0")
	(paper "A4")
	(lib_symbols
		(symbol "Device:LED"
			(pin_numbers hide)
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 0 2.54 0)
			)
			(property "Value" "LED"
				(at 0 -2.54 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Light emitting diode"
				(at 0 0 0)
			)
			(property "ki_keywords" "LED diode"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*"
				(at 0 0 0)
			)
			(symbol "LED_0_1"
				(polyline
					(pts
						(xy -1.27 -1.27) (xy -1.27 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 0) (xy 1.27 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -1.27) (xy 1.27 1.27) (xy -1.27 0) (xy 1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.048 -0.762) (xy -4.572 -2.286) (xy -3.81 -2.286) (xy -4.572 -2.286) (xy -4.572 -1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.778 -0.762) (xy -3.302 -2.286) (xy -2.54 -2.286) (xy -3.302 -2.286) (xy -3.302 -1.524)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "LED_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "K")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "A")
					(number "2")
				)
			)
		)
		(symbol "Device:R"
			(pin_numbers hide)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R"
				(at 0 0 90)
			)
			(property "Footprint" ""
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "MCU_RaspberryPi_and_Boards:Pico"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -13.97 27.94 0)
			)
			(property "Value" "Pico"
				(at 0 19.05 0)
			)
			(property "Footprint" "RPi_Pico:RPi_Pico_SMD_TH"
				(at 0 0 90)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(symbol "Pico_0_0"
				(text "Raspberry Pi Pico"
					(at 0 21.59 0)
				)
			)
			(symbol "Pico_0_1"
				(rectangle
					(start -15.24 26.67)
					(end 15.24 -26.67)
					(fill
						(type background)
					)
				)
			)
			(symbol "Pico_1_1"
				(pin bidirectional line
					(at -17.78 24.13 0)
					(length 2.54)
					(name "GPIO0")
					(number "1")
				)
				(pin bidirectional line
					(at -17.78 1.27 0)
					(length 2.54)
					(name "GPIO7")
					(number "10")
				)
				(pin bidirectional line
					(at -17.78 -1.27 0)
					(length 2.54)
					(name "GPIO8")
					(number "11")
				)
				(pin bidirectional line
					(at -17.78 -3.81 0)
					(length 2.54)
					(name "GPIO9")
					(number "12")
				)
				(pin power_in line
					(at -17.78 -6.35 0)
					(length 2.54)
					(name "GND")
					(number "13")
				)
				(pin bidirectional line
					(at -17.78 -8.89 0)
					(length 2.54)
					(name "GPIO10")
					(number "14")
				)
				(pin bidirectional line
					(at -17.78 -11.43 0)
					(length 2.54)
					(name "GPIO11")
					(number "15")
				)
				(pin bidirectional line
					(at -17.78 -13.97 0)
					(length 2.54)
					(name "GPIO12")
					(number "16")
				)
				(pin bidirectional line
					(at -17.78 -16.51 0)
					(length 2.54)
					(name "GPIO13")
					(number "17")
				)
				(pin power_in line
					(at -17.78 -19.05 0)
					(length 2.54)
					(name "GND")
					(number "18")
				)
				(pin bidirectional line
					(at -17.78 -21.59 0)
					(length 2.54)
					(name "GPIO14")
					(number "19")
				)
				(pin bidirectional line
					(at -17.78 21.59 0)
					(length 2.54)
					(name "GPIO1")
					(number "2")
				)
				(pin bidirectional line
					(at -17.78 -24.13 0)
					(length 2.54)
					(name "GPIO15")
					(number "20")
				)
				(pin bidirectional line
					(at 17.78 -24.13 180)
					(length 2.54)
					(name "GPIO16")
					(number "21")
				)
				(pin bidirectional line
					(at 17.78 -21.59 180)
					(length 2.54)
					(name "GPIO17")
					(number "22")
				)
				(pin power_in line
					(at 17.78 -19.05 180)
					(length 2.54)
					(name "GND")
					(number "23")
				)
				(pin bidirectional line
					(at 17.78 -16.51 180)
					(length 2.54)
					(name "GPIO18")
					(number "24")
				)
				(pin bidirectional line
					(at 17.78 -13.97 180)
					(length 2.54)
					(name "GPIO19")
					(number "25")
				)
				(pin bidirectional line
					(at 17.78 -11.43 180)
					(length 2.54)
					(name "GPIO20")
					(number "26")
				)
				(pin bidirectional line
					(at 17.78 -8.89 180)
					(length 2.54)
					(name "GPIO21")
					(number "27")
				)
				(pin power_in line
					(at 17.78 -6.35 180)
					(length 2.54)
					(name "GND")
					(number "28")
				)
				(pin bidirectional line
					(at 17.78 -3.81 180)
					(length 2.54)
					(name "GPIO22")
					(number "29")
				)
				(pin power_in line
					(at -17.78 19.05 0)
					(length 2.54)
					(name "GND")
					(number "3")
				)
				(pin input line
					(at 17.78 -1.27 180)
					(length 2.54)
					(name "RUN")
					(number "30")
				)
				(pin bidirectional line
					(at 17.78 1.27 180)
					(length 2.54)
					(name "GPIO26_ADC0")
					(number "31")
				)
				(pin bidirectional line
					(at 17.78 3.81 180)
					(length 2.54)
					(name "GPIO27_ADC1")
					(number "32")
				)
				(pin power_in line
					(at 17.78 6.35 180)
					(length 2.54)
					(name "AGND")
					(number "33")
				)
				(pin bidirectional line
					(at 17.78 8.89 180)
					(length 2.54)
					(name "GPIO28_ADC2")
					(number "34")
				)
				(pin power_in line
					(at 17.78 11.43 180)
					(length 2.54)
					(name "ADC_VREF")
					(number "35")
				)
				(pin power_in line
					(at 17.78 13.97 180)
					(length 2.54)
					(name "3V3")
					(number "36")
				)
				(pin input line
					(at 17.78 16.51 180)
					(length 2.54)
					(name "3V3_EN")
					(number "37")
				)
				(pin bidirectional line
					(at 17.78 19.05 180)
					(length 2.54)
					(name "GND")
					(number "38")
				)
				(pin power_in line
					(at 17.78 21.59 180)
					(length 2.54)
					(name "VSYS")
					(number "39")
				)
				(pin bidirectional line
					(at -17.78 16.51 0)
					(length 2.54)
					(name "GPIO2")
					(number "4")
				)
				(pin power_in line
					(at 17.78 24.13 180)
					(length 2.54)
					(name "VBUS")
					(number "40")
				)
				(pin input line
					(at -2.54 -29.21 90)
					(length 2.54)
					(name "SWCLK")
					(number "41")
				)
				(pin power_in line
					(at 0 -29.21 90)
					(length 2.54)
					(name "GND")
					(number "42")
				)
				(pin bidirectional line
					(at 2.54 -29.21 90)
					(length 2.54)
					(name "SWDIO")
					(number "43")
				)
				(pin bidirectional line
					(at -17.78 13.97 0)
					(length 2.54)
					(name "GPIO3")
					(number "5")
				)
				(pin bidirectional line
					(at -17.78 11.43 0)
					(length 2.54)
					(name "GPIO4")
					(number "6")
				)
				(pin bidirectional line
					(at -17.78 8.89 0)
					(length 2.54)
					(name "GPIO5")
					(number "7")
				)
				(pin power_in line
					(at -17.78 6.35 0)
					(length 2.54)
					(name "GND")
					(number "8")
				)
				(pin bidirectional line
					(at -17.78 3.81 0)
					(length 2.54)
					(name "GPIO6")
					(number "9")
				)
			)
		)
		(symbol "Switch:SW_Push"
			(pin_numbers hide)
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "SW"
				(at 1.27 2.54 0)
			)
			(property "Value" "SW_Push"
				(at 0 -1.524 0)
			)
			(property "Footprint" ""
				(at 0 5.08 0)
			)
			(property "Datasheet" "~"
				(at 0 5.08 0)
			)
			(property "Description" "Push button switch, generic, two pins"
				(at 0 0 0)
			)
			(property "ki_keywords" "switch normally-open pushbutton push-button"
				(at 0 0 0)
			)
			(symbol "SW_Push_0_1"
				(circle
					(center -2.032 0)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 1.27) (xy 0 3.048)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 1.27) (xy -2.54 1.27)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.032 0)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at -5.08 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
		)
		(symbol "power:Earth"
			(power)
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "Earth"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"Earth\""
				(at 0 0 0)
			)
			(property "ki_keywords" "global ground gnd"
				(at 0 0 0)
			)
			(symbol "Earth_0_1"
				(polyline
					(pts
						(xy -0.635 -1.905) (xy 0.635 -1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.127 -2.54) (xy 0.127 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -1.27) (xy 0 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -1.27) (xy -1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "Earth_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~")
					(number "1")
				)
			)
		)
	)
	(junction
		(at 167.64 101.6)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 157.48 101.6) (xy 167.64 101.6)
		)
	)
	(wire
		(pts
			(xy 157.48 99.06) (xy 157.48 101.6)
		)
	)
	(wire
		(pts
			(xy 175.26 92.71) (xy 175.26 90.17)
		)
	)
	(wire
		(pts
			(xy 167.64 101.6) (xy 175.26 101.6)
		)
	)
	(wire
		(pts
			(xy 157.48 83.82) (xy 157.48 88.9)
		)
	)
	(wire
		(pts
			(xy 148.59 81.28) (xy 167.64 81.28)
		)
	)
	(wire
		(pts
			(xy 175.26 78.74) (xy 148.59 78.74)
		)
	)
	(wire
		(pts
			(xy 175.26 100.33) (xy 175.26 101.6)
		)
	)
	(wire
		(pts
			(xy 175.26 78.74) (xy 175.26 82.55)
		)
	)
	(wire
		(pts
			(xy 167.64 81.28) (xy 167.64 101.6)
		)
	)
	(wire
		(pts
			(xy 148.59 83.82) (xy 157.48 83.82)
		)
	)
	(symbol
		(lib_id "MCU_RaspberryPi_and_Boards:Pico")
		(at 130.81 74.93 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U1"
			(at 130.81 43.18 0)
		)
		(property "Value" "Pico"
			(at 130.81 45.72 0)
		)
		(property "Footprint" "RPi_Pico:RPi_Pico_SMD_TH"
			(at 130.81 74.93 90)
		)
		(property "Datasheet" ""
			(at 130.81 74.93 0)
		)
		(property "Description" ""
			(at 130.81 74.93 0)
		)
		(pin "30")
		(pin "24")
		(pin "20")
		(pin "26")
		(pin "39")
		(pin "33")
		(pin "23")
		(pin "6")
		(pin "43")
		(pin "28")
		(pin "19")
		(pin "32")
		(pin "34")
		(pin "1")
		(pin "12")
		(pin "11")
		(pin "10")
		(pin "2")
		(pin "14")
		(pin "40")
		(pin "13")
		(pin "4")
		(pin "41")
		(pin "27")
		(pin "16")
		(pin "8")
		(pin "37")
		(pin "42")
		(pin "15")
		(pin "21")
		(pin "22")
		(pin "9")
		(pin "31")
		(pin "35")
		(pin "18")
		(pin "3")
		(pin "29")
		(pin "36")
		(pin "5")
		(pin "25")
		(pin "17")
		(pin "38")
		(pin "7")
		(instances
			(project ""
				(path
					(reference "U1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 175.26 96.52 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R1"
			(at 181.991 96.393 0)
		)
		(property "Value" "200 Ω"
			(at 185.293 99.187 0)
		)
		(property "Footprint" ""
			(at 177.038 96.52 90)
		)
		(property "Datasheet" "~"
			(at 175.26 96.52 0)
		)
		(property "Description" "Resistor"
			(at 175.26 96.52 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:Earth")
		(at 167.64 101.6 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01"
			(at 167.64 107.95 0)
		)
		(property "Value" "Earth"
			(at 167.64 106.68 0)
		)
		(property "Footprint" ""
			(at 167.64 101.6 0)
		)
		(property "Datasheet" "~"
			(at 167.64 101.6 0)
		)
		(property "Description" "Power symbol creates a global label with name \"Earth\""
			(at 167.64 101.6 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR01")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:LED")
		(at 175.26 86.36 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "D1"
			(at 182.499 89.027 90)
		)
		(property "Value" "LED"
			(at 181.737 85.471 90)
		)
		(property "Footprint" ""
			(at 175.26 86.36 0)
		)
		(property "Datasheet" "~"
			(at 175.26 86.36 0)
		)
		(property "Description" "Light emitting diode"
			(at 175.26 86.36 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "D1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 157.48 93.98 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW1"
			(at 161.29 92.7099 90)
		)
		(property "Value" "SW_Push"
			(at 161.29 95.2499 90)
		)
		(property "Footprint" ""
			(at 162.56 93.98 0)
		)
		(property "Datasheet" "~"
			(at 162.56 93.98 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 157.48 93.98 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "SW1")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
)
