(kicad_symbol_lib
	(version 20231120)
	(generator "kicad_symbol_editor")
	(generator_version "8.0")
	(symbol "LCD_Display_128x64_ST7920"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" ""
			(at 0 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "LCD_Display_128x64_ST7920_1_0"
			(text_box "Monochrome LCD display\nST7920"
				(at -36.83 -10.16 0)
				(size 71.12 -48.26)
				(fill
					(type color)
					(color 0 0 255 0.71)
				)
			)
		)
		(symbol "LCD_Display_128x64_ST7920_1_1"
			(pin power_in line
				(at 34.29 -71.12 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin bidirectional line
				(at 0 -71.12 90)
				(length 2.54)
				(name "DB3")
				(number "10")
			)
			(pin bidirectional line
				(at -3.81 -71.12 90)
				(length 2.54)
				(name "DB4")
				(number "11")
			)
			(pin bidirectional line
				(at -7.62 -71.12 90)
				(length 2.54)
				(name "DB5")
				(number "12")
			)
			(pin bidirectional line
				(at -11.43 -71.12 90)
				(length 2.54)
				(name "DB6")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 -71.12 90)
				(length 2.54)
				(name "DB7")
				(number "14")
			)
			(pin input line
				(at -19.05 -71.12 90)
				(length 2.54)
				(name "PSB")
				(number "15")
			)
			(pin no_connect line
				(at -22.86 -71.12 90)
				(length 2.54)
				(name "NC")
				(number "16")
			)
			(pin input line
				(at -26.67 -71.12 90)
				(length 2.54)
				(name "RTS")
				(number "17")
			)
			(pin power_out line
				(at -30.48 -71.12 90)
				(length 2.54)
				(name "VOUT")
				(number "18")
			)
			(pin power_in line
				(at -34.29 -71.12 90)
				(length 2.54)
				(name "BLA")
				(number "19")
			)
			(pin power_in line
				(at 30.48 -71.12 90)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at -38.1 -71.12 90)
				(length 2.54)
				(name "BLK")
				(number "20")
			)
			(pin power_out line
				(at 26.67 -71.12 90)
				(length 2.54)
				(name "VO")
				(number "3")
			)
			(pin input line
				(at 22.86 -71.12 90)
				(length 2.54)
				(name "RS")
				(number "4")
			)
			(pin input line
				(at 19.05 -71.12 90)
				(length 2.54)
				(name "P/W")
				(number "5")
			)
			(pin input line
				(at 15.24 -71.12 90)
				(length 2.54)
				(name "E")
				(number "6")
			)
			(pin bidirectional line
				(at 11.43 -71.12 90)
				(length 2.54)
				(name "DB0")
				(number "7")
			)
			(pin bidirectional line
				(at 7.62 -71.12 90)
				(length 2.54)
				(name "DB1")
				(number "8")
			)
			(pin bidirectional line
				(at 3.81 -71.12 90)
				(length 2.54)
				(name "DB2")
				(number "9")
			)
		)
	)
)
