(kicad_sch
	(version 20231120)
	(generator "eeschema")
	(generator_version "8.0")
	(paper "A4")
	(lib_symbols
		(symbol "Device:R"
			(pin_numbers hide)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R"
				(at 0 0 90)
			)
			(property "Footprint" ""
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "MCU_RaspberryPi_and_Boards:Pico"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -13.97 27.94 0)
			)
			(property "Value" "Pico"
				(at 0 19.05 0)
			)
			(property "Footprint" "RPi_Pico:RPi_Pico_SMD_TH"
				(at 0 0 90)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(symbol "Pico_0_0"
				(text "Raspberry Pi Pico"
					(at 0 21.59 0)
				)
			)
			(symbol "Pico_0_1"
				(rectangle
					(start -15.24 26.67)
					(end 15.24 -26.67)
					(fill
						(type background)
					)
				)
			)
			(symbol "Pico_1_1"
				(pin bidirectional line
					(at -17.78 24.13 0)
					(length 2.54)
					(name "GPIO0")
					(number "1")
				)
				(pin bidirectional line
					(at -17.78 1.27 0)
					(length 2.54)
					(name "GPIO7")
					(number "10")
				)
				(pin bidirectional line
					(at -17.78 -1.27 0)
					(length 2.54)
					(name "GPIO8")
					(number "11")
				)
				(pin bidirectional line
					(at -17.78 -3.81 0)
					(length 2.54)
					(name "GPIO9")
					(number "12")
				)
				(pin power_in line
					(at -17.78 -6.35 0)
					(length 2.54)
					(name "GND")
					(number "13")
				)
				(pin bidirectional line
					(at -17.78 -8.89 0)
					(length 2.54)
					(name "GPIO10")
					(number "14")
				)
				(pin bidirectional line
					(at -17.78 -11.43 0)
					(length 2.54)
					(name "GPIO11")
					(number "15")
				)
				(pin bidirectional line
					(at -17.78 -13.97 0)
					(length 2.54)
					(name "GPIO12")
					(number "16")
				)
				(pin bidirectional line
					(at -17.78 -16.51 0)
					(length 2.54)
					(name "GPIO13")
					(number "17")
				)
				(pin power_in line
					(at -17.78 -19.05 0)
					(length 2.54)
					(name "GND")
					(number "18")
				)
				(pin bidirectional line
					(at -17.78 -21.59 0)
					(length 2.54)
					(name "GPIO14")
					(number "19")
				)
				(pin bidirectional line
					(at -17.78 21.59 0)
					(length 2.54)
					(name "GPIO1")
					(number "2")
				)
				(pin bidirectional line
					(at -17.78 -24.13 0)
					(length 2.54)
					(name "GPIO15")
					(number "20")
				)
				(pin bidirectional line
					(at 17.78 -24.13 180)
					(length 2.54)
					(name "GPIO16")
					(number "21")
				)
				(pin bidirectional line
					(at 17.78 -21.59 180)
					(length 2.54)
					(name "GPIO17")
					(number "22")
				)
				(pin power_in line
					(at 17.78 -19.05 180)
					(length 2.54)
					(name "GND")
					(number "23")
				)
				(pin bidirectional line
					(at 17.78 -16.51 180)
					(length 2.54)
					(name "GPIO18")
					(number "24")
				)
				(pin bidirectional line
					(at 17.78 -13.97 180)
					(length 2.54)
					(name "GPIO19")
					(number "25")
				)
				(pin bidirectional line
					(at 17.78 -11.43 180)
					(length 2.54)
					(name "GPIO20")
					(number "26")
				)
				(pin bidirectional line
					(at 17.78 -8.89 180)
					(length 2.54)
					(name "GPIO21")
					(number "27")
				)
				(pin power_in line
					(at 17.78 -6.35 180)
					(length 2.54)
					(name "GND")
					(number "28")
				)
				(pin bidirectional line
					(at 17.78 -3.81 180)
					(length 2.54)
					(name "GPIO22")
					(number "29")
				)
				(pin power_in line
					(at -17.78 19.05 0)
					(length 2.54)
					(name "GND")
					(number "3")
				)
				(pin input line
					(at 17.78 -1.27 180)
					(length 2.54)
					(name "RUN")
					(number "30")
				)
				(pin bidirectional line
					(at 17.78 1.27 180)
					(length 2.54)
					(name "GPIO26_ADC0")
					(number "31")
				)
				(pin bidirectional line
					(at 17.78 3.81 180)
					(length 2.54)
					(name "GPIO27_ADC1")
					(number "32")
				)
				(pin power_in line
					(at 17.78 6.35 180)
					(length 2.54)
					(name "AGND")
					(number "33")
				)
				(pin bidirectional line
					(at 17.78 8.89 180)
					(length 2.54)
					(name "GPIO28_ADC2")
					(number "34")
				)
				(pin power_in line
					(at 17.78 11.43 180)
					(length 2.54)
					(name "ADC_VREF")
					(number "35")
				)
				(pin power_in line
					(at 17.78 13.97 180)
					(length 2.54)
					(name "3V3")
					(number "36")
				)
				(pin input line
					(at 17.78 16.51 180)
					(length 2.54)
					(name "3V3_EN")
					(number "37")
				)
				(pin bidirectional line
					(at 17.78 19.05 180)
					(length 2.54)
					(name "GND")
					(number "38")
				)
				(pin power_in line
					(at 17.78 21.59 180)
					(length 2.54)
					(name "VSYS")
					(number "39")
				)
				(pin bidirectional line
					(at -17.78 16.51 0)
					(length 2.54)
					(name "GPIO2")
					(number "4")
				)
				(pin power_in line
					(at 17.78 24.13 180)
					(length 2.54)
					(name "VBUS")
					(number "40")
				)
				(pin input line
					(at -2.54 -29.21 90)
					(length 2.54)
					(name "SWCLK")
					(number "41")
				)
				(pin power_in line
					(at 0 -29.21 90)
					(length 2.54)
					(name "GND")
					(number "42")
				)
				(pin bidirectional line
					(at 2.54 -29.21 90)
					(length 2.54)
					(name "SWDIO")
					(number "43")
				)
				(pin bidirectional line
					(at -17.78 13.97 0)
					(length 2.54)
					(name "GPIO3")
					(number "5")
				)
				(pin bidirectional line
					(at -17.78 11.43 0)
					(length 2.54)
					(name "GPIO4")
					(number "6")
				)
				(pin bidirectional line
					(at -17.78 8.89 0)
					(length 2.54)
					(name "GPIO5")
					(number "7")
				)
				(pin power_in line
					(at -17.78 6.35 0)
					(length 2.54)
					(name "GND")
					(number "8")
				)
				(pin bidirectional line
					(at -17.78 3.81 0)
					(length 2.54)
					(name "GPIO6")
					(number "9")
				)
			)
		)
		(symbol "Switch:SW_Push"
			(pin_numbers hide)
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "SW"
				(at 1.27 2.54 0)
			)
			(property "Value" "SW_Push"
				(at 0 -1.524 0)
			)
			(property "Footprint" ""
				(at 0 5.08 0)
			)
			(property "Datasheet" "~"
				(at 0 5.08 0)
			)
			(property "Description" "Push button switch, generic, two pins"
				(at 0 0 0)
			)
			(property "ki_keywords" "switch normally-open pushbutton push-button"
				(at 0 0 0)
			)
			(symbol "SW_Push_0_1"
				(circle
					(center -2.032 0)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 1.27) (xy 0 3.048)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 1.27) (xy -2.54 1.27)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.032 0)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at -5.08 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
		)
	)
	(junction
		(at 50.8 62.23)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 80.01 99.06)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 86.36 76.2)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 55.88 111.76)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 50.8 76.2)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 55.88 72.39)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 63.5 101.6)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 74.93 101.6)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 86.36 62.23)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 68.58 99.06)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 86.36 101.6)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 55.88 99.06)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 68.58 86.36)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 80.01 86.36)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 63.5 62.23)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 63.5 76.2)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 80.01 72.39)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 68.58 72.39)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 74.93 62.23)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 44.45 99.06)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 44.45 86.36)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 74.93 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 80.01 111.76)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 63.5 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 68.58 111.76)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 44.45 111.76)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 50.8 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 55.88 86.36)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 86.36 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 74.93 76.2)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 50.8 101.6)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 44.45 72.39)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 116.84 93.98) (xy 121.92 93.98)
		)
	)
	(wire
		(pts
			(xy 104.14 73.66) (xy 104.14 62.23)
		)
	)
	(wire
		(pts
			(xy 50.8 101.6) (xy 63.5 101.6)
		)
	)
	(wire
		(pts
			(xy 68.58 86.36) (xy 74.93 86.36)
		)
	)
	(wire
		(pts
			(xy 63.5 101.6) (xy 74.93 101.6)
		)
	)
	(wire
		(pts
			(xy 55.88 72.39) (xy 63.5 72.39)
		)
	)
	(wire
		(pts
			(xy 50.8 76.2) (xy 63.5 76.2)
		)
	)
	(wire
		(pts
			(xy 86.36 76.2) (xy 101.6 76.2)
		)
	)
	(wire
		(pts
			(xy 55.88 111.76) (xy 55.88 119.38)
		)
	)
	(wire
		(pts
			(xy 40.64 88.9) (xy 50.8 88.9)
		)
	)
	(wire
		(pts
			(xy 74.93 101.6) (xy 86.36 101.6)
		)
	)
	(wire
		(pts
			(xy 55.88 72.39) (xy 55.88 86.36)
		)
	)
	(wire
		(pts
			(xy 116.84 73.66) (xy 121.92 73.66)
		)
	)
	(wire
		(pts
			(xy 161.29 93.98) (xy 157.48 93.98)
		)
	)
	(wire
		(pts
			(xy 44.45 111.76) (xy 50.8 111.76)
		)
	)
	(wire
		(pts
			(xy 68.58 111.76) (xy 68.58 121.92)
		)
	)
	(wire
		(pts
			(xy 80.01 86.36) (xy 80.01 99.06)
		)
	)
	(wire
		(pts
			(xy 86.36 101.6) (xy 104.14 101.6)
		)
	)
	(wire
		(pts
			(xy 63.5 76.2) (xy 74.93 76.2)
		)
	)
	(wire
		(pts
			(xy 40.64 76.2) (xy 50.8 76.2)
		)
	)
	(wire
		(pts
			(xy 63.5 62.23) (xy 74.93 62.23)
		)
	)
	(wire
		(pts
			(xy 55.88 119.38) (xy 114.3 119.38)
		)
	)
	(wire
		(pts
			(xy 161.29 124.46) (xy 161.29 93.98)
		)
	)
	(wire
		(pts
			(xy 116.84 121.92) (xy 116.84 93.98)
		)
	)
	(wire
		(pts
			(xy 55.88 57.15) (xy 55.88 72.39)
		)
	)
	(wire
		(pts
			(xy 80.01 111.76) (xy 80.01 124.46)
		)
	)
	(wire
		(pts
			(xy 44.45 72.39) (xy 50.8 72.39)
		)
	)
	(wire
		(pts
			(xy 55.88 99.06) (xy 55.88 111.76)
		)
	)
	(wire
		(pts
			(xy 68.58 111.76) (xy 74.93 111.76)
		)
	)
	(wire
		(pts
			(xy 50.8 62.23) (xy 63.5 62.23)
		)
	)
	(wire
		(pts
			(xy 44.45 86.36) (xy 50.8 86.36)
		)
	)
	(wire
		(pts
			(xy 74.93 76.2) (xy 86.36 76.2)
		)
	)
	(wire
		(pts
			(xy 68.58 99.06) (xy 74.93 99.06)
		)
	)
	(wire
		(pts
			(xy 63.5 88.9) (xy 74.93 88.9)
		)
	)
	(wire
		(pts
			(xy 68.58 57.15) (xy 68.58 72.39)
		)
	)
	(wire
		(pts
			(xy 74.93 88.9) (xy 86.36 88.9)
		)
	)
	(wire
		(pts
			(xy 50.8 88.9) (xy 63.5 88.9)
		)
	)
	(wire
		(pts
			(xy 44.45 57.15) (xy 44.45 72.39)
		)
	)
	(wire
		(pts
			(xy 44.45 111.76) (xy 44.45 115.57)
		)
	)
	(wire
		(pts
			(xy 68.58 86.36) (xy 68.58 99.06)
		)
	)
	(wire
		(pts
			(xy 55.88 86.36) (xy 55.88 99.06)
		)
	)
	(wire
		(pts
			(xy 109.22 73.66) (xy 104.14 73.66)
		)
	)
	(wire
		(pts
			(xy 68.58 121.92) (xy 116.84 121.92)
		)
	)
	(wire
		(pts
			(xy 111.76 86.36) (xy 121.92 86.36)
		)
	)
	(wire
		(pts
			(xy 116.84 83.82) (xy 121.92 83.82)
		)
	)
	(wire
		(pts
			(xy 55.88 86.36) (xy 63.5 86.36)
		)
	)
	(wire
		(pts
			(xy 80.01 111.76) (xy 86.36 111.76)
		)
	)
	(wire
		(pts
			(xy 104.14 101.6) (xy 104.14 83.82)
		)
	)
	(wire
		(pts
			(xy 104.14 83.82) (xy 109.22 83.82)
		)
	)
	(wire
		(pts
			(xy 80.01 124.46) (xy 161.29 124.46)
		)
	)
	(wire
		(pts
			(xy 80.01 99.06) (xy 80.01 111.76)
		)
	)
	(wire
		(pts
			(xy 80.01 72.39) (xy 86.36 72.39)
		)
	)
	(wire
		(pts
			(xy 80.01 99.06) (xy 86.36 99.06)
		)
	)
	(wire
		(pts
			(xy 44.45 72.39) (xy 44.45 86.36)
		)
	)
	(wire
		(pts
			(xy 80.01 57.15) (xy 80.01 72.39)
		)
	)
	(wire
		(pts
			(xy 44.45 86.36) (xy 44.45 99.06)
		)
	)
	(wire
		(pts
			(xy 44.45 99.06) (xy 50.8 99.06)
		)
	)
	(wire
		(pts
			(xy 101.6 81.28) (xy 101.6 88.9)
		)
	)
	(wire
		(pts
			(xy 116.84 81.28) (xy 121.92 81.28)
		)
	)
	(wire
		(pts
			(xy 74.93 62.23) (xy 86.36 62.23)
		)
	)
	(wire
		(pts
			(xy 44.45 115.57) (xy 111.76 115.57)
		)
	)
	(wire
		(pts
			(xy 111.76 115.57) (xy 111.76 86.36)
		)
	)
	(wire
		(pts
			(xy 116.84 78.74) (xy 121.92 78.74)
		)
	)
	(wire
		(pts
			(xy 80.01 86.36) (xy 86.36 86.36)
		)
	)
	(wire
		(pts
			(xy 109.22 78.74) (xy 101.6 78.74)
		)
	)
	(wire
		(pts
			(xy 55.88 99.06) (xy 63.5 99.06)
		)
	)
	(wire
		(pts
			(xy 44.45 99.06) (xy 44.45 111.76)
		)
	)
	(wire
		(pts
			(xy 109.22 81.28) (xy 101.6 81.28)
		)
	)
	(wire
		(pts
			(xy 40.64 101.6) (xy 50.8 101.6)
		)
	)
	(wire
		(pts
			(xy 80.01 72.39) (xy 80.01 86.36)
		)
	)
	(wire
		(pts
			(xy 55.88 111.76) (xy 63.5 111.76)
		)
	)
	(wire
		(pts
			(xy 68.58 99.06) (xy 68.58 111.76)
		)
	)
	(wire
		(pts
			(xy 68.58 72.39) (xy 74.93 72.39)
		)
	)
	(wire
		(pts
			(xy 114.3 119.38) (xy 114.3 91.44)
		)
	)
	(wire
		(pts
			(xy 101.6 78.74) (xy 101.6 76.2)
		)
	)
	(wire
		(pts
			(xy 114.3 91.44) (xy 121.92 91.44)
		)
	)
	(wire
		(pts
			(xy 86.36 88.9) (xy 101.6 88.9)
		)
	)
	(wire
		(pts
			(xy 86.36 62.23) (xy 104.14 62.23)
		)
	)
	(wire
		(pts
			(xy 40.64 62.23) (xy 50.8 62.23)
		)
	)
	(wire
		(pts
			(xy 68.58 72.39) (xy 68.58 86.36)
		)
	)
	(text "8"
		(exclude_from_sim no)
		(at 66.04 94.488 0)
	)
	(text "9"
		(exclude_from_sim no)
		(at 77.47 94.742 0)
	)
	(text "GPIO výstupy"
		(exclude_from_sim no)
		(at 23.876 83.058 0)
	)
	(text "3"
		(exclude_from_sim no)
		(at 76.962 67.818 0)
	)
	(text "*"
		(exclude_from_sim no)
		(at 53.086 107.188 0)
	)
	(text "7"
		(exclude_from_sim no)
		(at 53.086 94.488 0)
	)
	(text "6"
		(exclude_from_sim no)
		(at 77.47 81.534 0)
	)
	(text "2"
		(exclude_from_sim no)
		(at 65.786 67.818 0)
	)
	(text "1"
		(exclude_from_sim no)
		(at 52.832 67.564 0)
	)
	(text "0"
		(exclude_from_sim no)
		(at 65.532 107.188 0)
	)
	(text "GPIO vstupy"
		(exclude_from_sim no)
		(at 66.294 42.418 0)
	)
	(text "#"
		(exclude_from_sim no)
		(at 77.47 106.68 0)
	)
	(text "C"
		(exclude_from_sim no)
		(at 89.154 94.234 0)
	)
	(text "A"
		(exclude_from_sim no)
		(at 89.916 67.818 0)
	)
	(text "4"
		(exclude_from_sim no)
		(at 53.34 81.788 0)
	)
	(text "5"
		(exclude_from_sim no)
		(at 65.532 82.042 0)
	)
	(text "B"
		(exclude_from_sim no)
		(at 89.154 82.042 0)
	)
	(text "D"
		(exclude_from_sim no)
		(at 88.9 107.188 0)
	)
	(global_label "GPIO14"
		(shape input)
		(at 55.88 57.15 90)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 55.88 47.2705 90)
		)
	)
	(global_label "GPIO9"
		(shape input)
		(at 40.64 62.23 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 31.97 62.23 0)
		)
	)
	(global_label "GPIO12"
		(shape input)
		(at 40.64 101.6 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 30.7605 101.6 0)
		)
	)
	(global_label "GPIO16"
		(shape input)
		(at 80.01 57.15 90)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 80.01 47.2705 90)
		)
	)
	(global_label "GPIO11"
		(shape input)
		(at 40.64 88.9 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 30.7605 88.9 0)
		)
	)
	(global_label "GPIO15"
		(shape input)
		(at 68.58 57.15 90)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 68.58 47.2705 90)
		)
	)
	(global_label "GPIO10"
		(shape input)
		(at 40.64 76.2 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 30.7605 76.2 0)
		)
	)
	(global_label "GPIO13"
		(shape input)
		(at 44.45 57.15 90)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 44.45 47.2705 90)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 50.8 106.68 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW13"
			(at 52.07 105.4099 90)
		)
		(property "Value" "SW_Push"
			(at 52.07 107.9499 90)
		)
		(property "Footprint" ""
			(at 45.72 106.68 0)
		)
		(property "Datasheet" "~"
			(at 45.72 106.68 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 50.8 106.68 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "keypad4x4"
				(path
					(reference "SW13")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 50.8 81.28 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW5"
			(at 52.07 80.0099 90)
		)
		(property "Value" "SW_Push"
			(at 52.07 82.5499 90)
		)
		(property "Footprint" ""
			(at 45.72 81.28 0)
		)
		(property "Datasheet" "~"
			(at 45.72 81.28 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 50.8 81.28 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "keypad4x4"
				(path
					(reference "SW5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 74.93 106.68 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW15"
			(at 76.2 105.4099 90)
		)
		(property "Value" "SW_Push"
			(at 76.2 107.9499 90)
		)
		(property "Footprint" ""
			(at 69.85 106.68 0)
		)
		(property "Datasheet" "~"
			(at 69.85 106.68 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 74.93 106.68 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "keypad4x4"
				(path
					(reference "SW15")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 86.36 67.31 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW4"
			(at 87.63 66.0399 90)
		)
		(property "Value" "SW_Push"
			(at 87.63 68.5799 90)
		)
		(property "Footprint" ""
			(at 81.28 67.31 0)
		)
		(property "Datasheet" "~"
			(at 81.28 67.31 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 86.36 67.31 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "keypad4x4"
				(path
					(reference "SW4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 50.8 93.98 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW9"
			(at 52.07 92.7099 90)
		)
		(property "Value" "SW_Push"
			(at 52.07 95.2499 90)
		)
		(property "Footprint" ""
			(at 45.72 93.98 0)
		)
		(property "Datasheet" "~"
			(at 45.72 93.98 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 50.8 93.98 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "keypad4x4"
				(path
					(reference "SW9")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 113.03 83.82 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R1-R3"
			(at 113.03 77.47 90)
		)
		(property "Value" "330"
			(at 113.03 80.01 90)
		)
		(property "Footprint" ""
			(at 113.03 85.598 90)
		)
		(property "Datasheet" "~"
			(at 113.03 83.82 0)
		)
		(property "Description" "Resistor"
			(at 113.03 83.82 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "keypad4x4"
				(path
					(reference "R1-R3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 63.5 93.98 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW10"
			(at 64.77 92.7099 90)
		)
		(property "Value" "SW_Push"
			(at 64.77 95.2499 90)
		)
		(property "Footprint" ""
			(at 58.42 93.98 0)
		)
		(property "Datasheet" "~"
			(at 58.42 93.98 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 63.5 93.98 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "keypad4x4"
				(path
					(reference "SW10")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 86.36 93.98 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW12"
			(at 87.63 92.7099 90)
		)
		(property "Value" "SW_Push"
			(at 87.63 95.2499 90)
		)
		(property "Footprint" ""
			(at 81.28 93.98 0)
		)
		(property "Datasheet" "~"
			(at 81.28 93.98 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 86.36 93.98 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "keypad4x4"
				(path
					(reference "SW12")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 63.5 67.31 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW2"
			(at 64.77 66.0399 90)
		)
		(property "Value" "SW_Push"
			(at 64.77 68.5799 90)
		)
		(property "Footprint" ""
			(at 58.42 67.31 0)
		)
		(property "Datasheet" "~"
			(at 58.42 67.31 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 63.5 67.31 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "keypad4x4"
				(path
					(reference "SW2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 63.5 81.28 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW6"
			(at 64.77 80.0099 90)
		)
		(property "Value" "SW_Push"
			(at 64.77 82.5499 90)
		)
		(property "Footprint" ""
			(at 58.42 81.28 0)
		)
		(property "Datasheet" "~"
			(at 58.42 81.28 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 63.5 81.28 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "keypad4x4"
				(path
					(reference "SW6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 86.36 81.28 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW8"
			(at 87.63 80.0099 90)
		)
		(property "Value" "SW_Push"
			(at 87.63 82.5499 90)
		)
		(property "Footprint" ""
			(at 81.28 81.28 0)
		)
		(property "Datasheet" "~"
			(at 81.28 81.28 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 86.36 81.28 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "keypad4x4"
				(path
					(reference "SW8")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 86.36 106.68 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW16"
			(at 87.63 105.4099 90)
		)
		(property "Value" "SW_Push"
			(at 87.63 107.9499 90)
		)
		(property "Footprint" ""
			(at 81.28 106.68 0)
		)
		(property "Datasheet" "~"
			(at 81.28 106.68 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 86.36 106.68 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "keypad4x4"
				(path
					(reference "SW16")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 113.03 81.28 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R1-R2"
			(at 113.03 74.93 90)
		)
		(property "Value" "330"
			(at 113.03 77.47 90)
		)
		(property "Footprint" ""
			(at 113.03 83.058 90)
		)
		(property "Datasheet" "~"
			(at 113.03 81.28 0)
		)
		(property "Description" "Resistor"
			(at 113.03 81.28 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "keypad4x4"
				(path
					(reference "R1-R2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 113.03 78.74 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R1-R1"
			(at 113.03 72.39 90)
		)
		(property "Value" "330"
			(at 113.03 74.93 90)
		)
		(property "Footprint" ""
			(at 113.03 80.518 90)
		)
		(property "Datasheet" "~"
			(at 113.03 78.74 0)
		)
		(property "Description" "Resistor"
			(at 113.03 78.74 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "keypad4x4"
				(path
					(reference "R1-R1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 74.93 81.28 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW7"
			(at 76.2 80.0099 90)
		)
		(property "Value" "SW_Push"
			(at 76.2 82.5499 90)
		)
		(property "Footprint" ""
			(at 69.85 81.28 0)
		)
		(property "Datasheet" "~"
			(at 69.85 81.28 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 74.93 81.28 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "keypad4x4"
				(path
					(reference "SW7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 63.5 106.68 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW14"
			(at 64.77 105.4099 90)
		)
		(property "Value" "SW_Push"
			(at 64.77 107.9499 90)
		)
		(property "Footprint" ""
			(at 58.42 106.68 0)
		)
		(property "Datasheet" "~"
			(at 58.42 106.68 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 63.5 106.68 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "keypad4x4"
				(path
					(reference "SW14")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 74.93 67.31 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW3"
			(at 76.2 66.0399 90)
		)
		(property "Value" "SW_Push"
			(at 76.2 68.5799 90)
		)
		(property "Footprint" ""
			(at 69.85 67.31 0)
		)
		(property "Datasheet" "~"
			(at 69.85 67.31 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 74.93 67.31 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "keypad4x4"
				(path
					(reference "SW3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 113.03 73.66 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R1-R4"
			(at 113.03 67.31 90)
		)
		(property "Value" "330"
			(at 113.03 69.85 90)
		)
		(property "Footprint" ""
			(at 113.03 75.438 90)
		)
		(property "Datasheet" "~"
			(at 113.03 73.66 0)
		)
		(property "Description" "Resistor"
			(at 113.03 73.66 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "R1-R4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "MCU_RaspberryPi_and_Boards:Pico")
		(at 139.7 69.85 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U1"
			(at 139.7 38.1 0)
		)
		(property "Value" "Pico"
			(at 139.7 40.64 0)
		)
		(property "Footprint" "RPi_Pico:RPi_Pico_SMD_TH"
			(at 139.7 69.85 90)
		)
		(property "Datasheet" ""
			(at 139.7 69.85 0)
		)
		(property "Description" ""
			(at 139.7 69.85 0)
		)
		(pin "21")
		(pin "20")
		(pin "37")
		(pin "27")
		(pin "2")
		(pin "7")
		(pin "41")
		(pin "29")
		(pin "28")
		(pin "36")
		(pin "22")
		(pin "26")
		(pin "3")
		(pin "12")
		(pin "31")
		(pin "11")
		(pin "10")
		(pin "1")
		(pin "13")
		(pin "14")
		(pin "23")
		(pin "15")
		(pin "35")
		(pin "30")
		(pin "6")
		(pin "40")
		(pin "33")
		(pin "4")
		(pin "19")
		(pin "38")
		(pin "8")
		(pin "32")
		(pin "17")
		(pin "42")
		(pin "24")
		(pin "18")
		(pin "25")
		(pin "34")
		(pin "39")
		(pin "16")
		(pin "9")
		(pin "5")
		(pin "43")
		(instances
			(project ""
				(path
					(reference "U1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 50.8 67.31 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW1"
			(at 52.07 66.0399 90)
		)
		(property "Value" "SW_Push"
			(at 52.07 68.5799 90)
		)
		(property "Footprint" ""
			(at 45.72 67.31 0)
		)
		(property "Datasheet" "~"
			(at 45.72 67.31 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 50.8 67.31 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "SW1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 74.93 93.98 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW11"
			(at 76.2 92.7099 90)
		)
		(property "Value" "SW_Push"
			(at 76.2 95.2499 90)
		)
		(property "Footprint" ""
			(at 69.85 93.98 0)
		)
		(property "Datasheet" "~"
			(at 69.85 93.98 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 74.93 93.98 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "keypad4x4"
				(path
					(reference "SW11")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
)
