(kicad_sch
	(version 20231120)
	(generator "eeschema")
	(generator_version "8.0")
	(paper "A4")
	(title_block
		(title "Jednoduchá GPS navigace")
		(company "Jirka Chráska")
	)
	(lib_symbols
		(symbol "L76K:GPS_L76K_module"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "M"
				(at 0 0 0)
			)
			(property "Value" ""
				(at 0 0 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(symbol "GPS_L76K_module_1_1"
				(rectangle
					(start -5.08 -2.54)
					(end 5.08 -17.78)
					(fill
						(type background)
					)
				)
				(text "Waveshare GNSS L76K module"
					(at 10.16 -20.32 0)
				)
				(pin power_in line
					(at -7.62 -5.08 0)
					(length 2.54)
					(name "VCC")
					(number "1")
				)
				(pin power_in line
					(at -7.62 -7.62 0)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin output line
					(at -7.62 -10.16 0)
					(length 2.54)
					(name "TX")
					(number "3")
				)
				(pin input line
					(at -7.62 -12.7 0)
					(length 2.54)
					(name "RX")
					(number "4")
				)
				(pin output line
					(at -7.62 -15.24 0)
					(length 2.54)
					(name "PPS")
					(number "5")
				)
			)
		)
		(symbol "MCU_RaspberryPi_and_Boards:Pico"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -13.97 27.94 0)
			)
			(property "Value" "Pico"
				(at 0 19.05 0)
			)
			(property "Footprint" "RPi_Pico:RPi_Pico_SMD_TH"
				(at 0 0 90)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(symbol "Pico_0_0"
				(text "Raspberry Pi Pico"
					(at 0 21.59 0)
				)
			)
			(symbol "Pico_0_1"
				(rectangle
					(start -15.24 26.67)
					(end 15.24 -26.67)
					(fill
						(type background)
					)
				)
			)
			(symbol "Pico_1_1"
				(pin bidirectional line
					(at -17.78 24.13 0)
					(length 2.54)
					(name "GPIO0")
					(number "1")
				)
				(pin bidirectional line
					(at -17.78 1.27 0)
					(length 2.54)
					(name "GPIO7")
					(number "10")
				)
				(pin bidirectional line
					(at -17.78 -1.27 0)
					(length 2.54)
					(name "GPIO8")
					(number "11")
				)
				(pin bidirectional line
					(at -17.78 -3.81 0)
					(length 2.54)
					(name "GPIO9")
					(number "12")
				)
				(pin power_in line
					(at -17.78 -6.35 0)
					(length 2.54)
					(name "GND")
					(number "13")
				)
				(pin bidirectional line
					(at -17.78 -8.89 0)
					(length 2.54)
					(name "GPIO10")
					(number "14")
				)
				(pin bidirectional line
					(at -17.78 -11.43 0)
					(length 2.54)
					(name "GPIO11")
					(number "15")
				)
				(pin bidirectional line
					(at -17.78 -13.97 0)
					(length 2.54)
					(name "GPIO12")
					(number "16")
				)
				(pin bidirectional line
					(at -17.78 -16.51 0)
					(length 2.54)
					(name "GPIO13")
					(number "17")
				)
				(pin power_in line
					(at -17.78 -19.05 0)
					(length 2.54)
					(name "GND")
					(number "18")
				)
				(pin bidirectional line
					(at -17.78 -21.59 0)
					(length 2.54)
					(name "GPIO14")
					(number "19")
				)
				(pin bidirectional line
					(at -17.78 21.59 0)
					(length 2.54)
					(name "GPIO1")
					(number "2")
				)
				(pin bidirectional line
					(at -17.78 -24.13 0)
					(length 2.54)
					(name "GPIO15")
					(number "20")
				)
				(pin bidirectional line
					(at 17.78 -24.13 180)
					(length 2.54)
					(name "GPIO16")
					(number "21")
				)
				(pin bidirectional line
					(at 17.78 -21.59 180)
					(length 2.54)
					(name "GPIO17")
					(number "22")
				)
				(pin power_in line
					(at 17.78 -19.05 180)
					(length 2.54)
					(name "GND")
					(number "23")
				)
				(pin bidirectional line
					(at 17.78 -16.51 180)
					(length 2.54)
					(name "GPIO18")
					(number "24")
				)
				(pin bidirectional line
					(at 17.78 -13.97 180)
					(length 2.54)
					(name "GPIO19")
					(number "25")
				)
				(pin bidirectional line
					(at 17.78 -11.43 180)
					(length 2.54)
					(name "GPIO20")
					(number "26")
				)
				(pin bidirectional line
					(at 17.78 -8.89 180)
					(length 2.54)
					(name "GPIO21")
					(number "27")
				)
				(pin power_in line
					(at 17.78 -6.35 180)
					(length 2.54)
					(name "GND")
					(number "28")
				)
				(pin bidirectional line
					(at 17.78 -3.81 180)
					(length 2.54)
					(name "GPIO22")
					(number "29")
				)
				(pin power_in line
					(at -17.78 19.05 0)
					(length 2.54)
					(name "GND")
					(number "3")
				)
				(pin input line
					(at 17.78 -1.27 180)
					(length 2.54)
					(name "RUN")
					(number "30")
				)
				(pin bidirectional line
					(at 17.78 1.27 180)
					(length 2.54)
					(name "GPIO26_ADC0")
					(number "31")
				)
				(pin bidirectional line
					(at 17.78 3.81 180)
					(length 2.54)
					(name "GPIO27_ADC1")
					(number "32")
				)
				(pin power_in line
					(at 17.78 6.35 180)
					(length 2.54)
					(name "AGND")
					(number "33")
				)
				(pin bidirectional line
					(at 17.78 8.89 180)
					(length 2.54)
					(name "GPIO28_ADC2")
					(number "34")
				)
				(pin power_in line
					(at 17.78 11.43 180)
					(length 2.54)
					(name "ADC_VREF")
					(number "35")
				)
				(pin power_in line
					(at 17.78 13.97 180)
					(length 2.54)
					(name "3V3")
					(number "36")
				)
				(pin input line
					(at 17.78 16.51 180)
					(length 2.54)
					(name "3V3_EN")
					(number "37")
				)
				(pin bidirectional line
					(at 17.78 19.05 180)
					(length 2.54)
					(name "GND")
					(number "38")
				)
				(pin power_in line
					(at 17.78 21.59 180)
					(length 2.54)
					(name "VSYS")
					(number "39")
				)
				(pin bidirectional line
					(at -17.78 16.51 0)
					(length 2.54)
					(name "GPIO2")
					(number "4")
				)
				(pin power_in line
					(at 17.78 24.13 180)
					(length 2.54)
					(name "VBUS")
					(number "40")
				)
				(pin input line
					(at -2.54 -29.21 90)
					(length 2.54)
					(name "SWCLK")
					(number "41")
				)
				(pin power_in line
					(at 0 -29.21 90)
					(length 2.54)
					(name "GND")
					(number "42")
				)
				(pin bidirectional line
					(at 2.54 -29.21 90)
					(length 2.54)
					(name "SWDIO")
					(number "43")
				)
				(pin bidirectional line
					(at -17.78 13.97 0)
					(length 2.54)
					(name "GPIO3")
					(number "5")
				)
				(pin bidirectional line
					(at -17.78 11.43 0)
					(length 2.54)
					(name "GPIO4")
					(number "6")
				)
				(pin bidirectional line
					(at -17.78 8.89 0)
					(length 2.54)
					(name "GPIO5")
					(number "7")
				)
				(pin power_in line
					(at -17.78 6.35 0)
					(length 2.54)
					(name "GND")
					(number "8")
				)
				(pin bidirectional line
					(at -17.78 3.81 0)
					(length 2.54)
					(name "GPIO6")
					(number "9")
				)
			)
		)
		(symbol "Switch:SW_Push"
			(pin_numbers hide)
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "SW"
				(at 1.27 2.54 0)
			)
			(property "Value" "SW_Push"
				(at 0 -1.524 0)
			)
			(property "Footprint" ""
				(at 0 5.08 0)
			)
			(property "Datasheet" "~"
				(at 0 5.08 0)
			)
			(property "Description" "Push button switch, generic, two pins"
				(at 0 0 0)
			)
			(property "ki_keywords" "switch normally-open pushbutton push-button"
				(at 0 0 0)
			)
			(symbol "SW_Push_0_1"
				(circle
					(center -2.032 0)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 1.27) (xy 0 3.048)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 1.27) (xy -2.54 1.27)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.032 0)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at -5.08 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
		)
		(symbol "lcd_display_128x64_st7920:LCD_Display_128x64_ST7920"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 0 0 0)
			)
			(property "Value" ""
				(at 0 0 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(symbol "LCD_Display_128x64_ST7920_1_0"
				(text_box "Monochrome LCD display\nST7920"
					(at -36.83 -10.16 0)
					(size 71.12 -48.26)
					(fill
						(type color)
						(color 0 0 255 0.71)
					)
				)
			)
			(symbol "LCD_Display_128x64_ST7920_1_1"
				(rectangle
					(start -44.45 -3.81)
					(end 40.64 -68.58)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 34.29 -71.12 90)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -71.12 90)
					(length 2.54)
					(name "DB3")
					(number "10")
				)
				(pin bidirectional line
					(at -3.81 -71.12 90)
					(length 2.54)
					(name "DB4")
					(number "11")
				)
				(pin bidirectional line
					(at -7.62 -71.12 90)
					(length 2.54)
					(name "DB5")
					(number "12")
				)
				(pin bidirectional line
					(at -11.43 -71.12 90)
					(length 2.54)
					(name "DB6")
					(number "13")
				)
				(pin bidirectional line
					(at -15.24 -71.12 90)
					(length 2.54)
					(name "DB7")
					(number "14")
				)
				(pin input line
					(at -19.05 -71.12 90)
					(length 2.54)
					(name "PSB")
					(number "15")
				)
				(pin no_connect line
					(at -22.86 -71.12 90)
					(length 2.54)
					(name "NC")
					(number "16")
				)
				(pin input line
					(at -26.67 -71.12 90)
					(length 2.54)
					(name "RTS")
					(number "17")
				)
				(pin power_out line
					(at -30.48 -71.12 90)
					(length 2.54)
					(name "VOUT")
					(number "18")
				)
				(pin power_in line
					(at -34.29 -71.12 90)
					(length 2.54)
					(name "BLA")
					(number "19")
				)
				(pin power_in line
					(at 30.48 -71.12 90)
					(length 2.54)
					(name "VCC")
					(number "2")
				)
				(pin power_in line
					(at -38.1 -71.12 90)
					(length 2.54)
					(name "BLK")
					(number "20")
				)
				(pin power_out line
					(at 26.67 -71.12 90)
					(length 2.54)
					(name "VO")
					(number "3")
				)
				(pin input line
					(at 22.86 -71.12 90)
					(length 2.54)
					(name "RS")
					(number "4")
				)
				(pin input line
					(at 19.05 -71.12 90)
					(length 2.54)
					(name "P/W")
					(number "5")
				)
				(pin input line
					(at 15.24 -71.12 90)
					(length 2.54)
					(name "E")
					(number "6")
				)
				(pin bidirectional line
					(at 11.43 -71.12 90)
					(length 2.54)
					(name "DB0")
					(number "7")
				)
				(pin bidirectional line
					(at 7.62 -71.12 90)
					(length 2.54)
					(name "DB1")
					(number "8")
				)
				(pin bidirectional line
					(at 3.81 -71.12 90)
					(length 2.54)
					(name "DB2")
					(number "9")
				)
			)
		)
		(symbol "power:GNDD"
			(power)
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GNDD"
				(at 0 -3.175 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GNDD\" , digital ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "GNDD_0_1"
				(rectangle
					(start -1.27 -1.524)
					(end 1.27 -2.032)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.524)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GNDD_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~")
					(number "1")
				)
			)
		)
	)
	(junction
		(at 107.95 118.11)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 111.76 120.65)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 111.76 87.63) (xy 111.76 120.65)
		)
	)
	(wire
		(pts
			(xy 24.13 97.79) (xy 24.13 156.21)
		)
	)
	(wire
		(pts
			(xy 24.13 156.21) (xy 38.1 156.21)
		)
	)
	(wire
		(pts
			(xy 86.36 143.51) (xy 73.66 143.51)
		)
	)
	(wire
		(pts
			(xy 123.19 110.49) (xy 123.19 125.73)
		)
	)
	(wire
		(pts
			(xy 123.19 125.73) (xy 133.35 125.73)
		)
	)
	(wire
		(pts
			(xy 26.67 100.33) (xy 26.67 123.19)
		)
	)
	(wire
		(pts
			(xy 73.66 148.59) (xy 93.98 148.59)
		)
	)
	(wire
		(pts
			(xy 96.52 102.87) (xy 29.21 102.87)
		)
	)
	(wire
		(pts
			(xy 104.14 125.73) (xy 104.14 148.59)
		)
	)
	(wire
		(pts
			(xy 50.8 97.79) (xy 24.13 97.79)
		)
	)
	(wire
		(pts
			(xy 35.56 118.11) (xy 35.56 107.95)
		)
	)
	(wire
		(pts
			(xy 38.1 110.49) (xy 123.19 110.49)
		)
	)
	(wire
		(pts
			(xy 31.75 105.41) (xy 31.75 130.81)
		)
	)
	(wire
		(pts
			(xy 125.73 123.19) (xy 133.35 123.19)
		)
	)
	(wire
		(pts
			(xy 43.18 93.98) (xy 86.36 93.98)
		)
	)
	(wire
		(pts
			(xy 43.18 87.63) (xy 43.18 93.98)
		)
	)
	(wire
		(pts
			(xy 31.75 130.81) (xy 38.1 130.81)
		)
	)
	(wire
		(pts
			(xy 29.21 125.73) (xy 38.1 125.73)
		)
	)
	(wire
		(pts
			(xy 92.71 87.63) (xy 92.71 100.33)
		)
	)
	(wire
		(pts
			(xy 107.95 118.11) (xy 133.35 118.11)
		)
	)
	(wire
		(pts
			(xy 100.33 87.63) (xy 100.33 105.41)
		)
	)
	(wire
		(pts
			(xy 111.76 120.65) (xy 73.66 120.65)
		)
	)
	(wire
		(pts
			(xy 96.52 87.63) (xy 96.52 102.87)
		)
	)
	(wire
		(pts
			(xy 111.76 125.73) (xy 111.76 120.65)
		)
	)
	(wire
		(pts
			(xy 26.67 123.19) (xy 38.1 123.19)
		)
	)
	(wire
		(pts
			(xy 38.1 118.11) (xy 35.56 118.11)
		)
	)
	(wire
		(pts
			(xy 107.95 87.63) (xy 107.95 118.11)
		)
	)
	(wire
		(pts
			(xy 86.36 93.98) (xy 86.36 143.51)
		)
	)
	(wire
		(pts
			(xy 100.33 105.41) (xy 31.75 105.41)
		)
	)
	(wire
		(pts
			(xy 38.1 115.57) (xy 38.1 110.49)
		)
	)
	(wire
		(pts
			(xy 50.8 87.63) (xy 50.8 97.79)
		)
	)
	(wire
		(pts
			(xy 92.71 100.33) (xy 26.67 100.33)
		)
	)
	(wire
		(pts
			(xy 35.56 107.95) (xy 125.73 107.95)
		)
	)
	(wire
		(pts
			(xy 111.76 120.65) (xy 133.35 120.65)
		)
	)
	(wire
		(pts
			(xy 29.21 102.87) (xy 29.21 125.73)
		)
	)
	(wire
		(pts
			(xy 73.66 118.11) (xy 107.95 118.11)
		)
	)
	(wire
		(pts
			(xy 125.73 107.95) (xy 125.73 123.19)
		)
	)
	(wire
		(pts
			(xy 73.66 125.73) (xy 104.14 125.73)
		)
	)
	(text "5V"
		(exclude_from_sim no)
		(at 90.932 116.84 0)
	)
	(symbol
		(lib_id "power:GNDD")
		(at 111.76 125.73 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01"
			(at 111.76 132.08 0)
		)
		(property "Value" "GND"
			(at 114.3 126.8094 0)
		)
		(property "Footprint" ""
			(at 111.76 125.73 0)
		)
		(property "Datasheet" ""
			(at 111.76 125.73 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GNDD\" , digital ground"
			(at 111.76 125.73 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR01")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "MCU_RaspberryPi_and_Boards:Pico")
		(at 55.88 139.7 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "U1"
			(at 56.134 122.682 0)
		)
		(property "Value" "Pico"
			(at 56.134 125.222 0)
		)
		(property "Footprint" "RPi_Pico:RPi_Pico_SMD_TH"
			(at 55.88 139.7 90)
		)
		(property "Datasheet" ""
			(at 55.88 139.7 0)
		)
		(property "Description" ""
			(at 55.88 139.7 0)
		)
		(pin "19")
		(pin "21")
		(pin "23")
		(pin "1")
		(pin "12")
		(pin "11")
		(pin "10")
		(pin "35")
		(pin "4")
		(pin "29")
		(pin "13")
		(pin "3")
		(pin "39")
		(pin "28")
		(pin "7")
		(pin "8")
		(pin "20")
		(pin "9")
		(pin "42")
		(pin "22")
		(pin "30")
		(pin "25")
		(pin "38")
		(pin "33")
		(pin "6")
		(pin "36")
		(pin "32")
		(pin "34")
		(pin "40")
		(pin "37")
		(pin "43")
		(pin "41")
		(pin "15")
		(pin "17")
		(pin "2")
		(pin "24")
		(pin "31")
		(pin "5")
		(pin "27")
		(pin "18")
		(pin "14")
		(pin "26")
		(pin "16")
		(instances
			(project ""
				(path
					(reference "U1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 99.06 148.59 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "TL1"
			(at 99.06 142.24 0)
		)
		(property "Value" "~"
			(at 99.06 143.51 0)
		)
		(property "Footprint" ""
			(at 99.06 143.51 0)
		)
		(property "Datasheet" "~"
			(at 99.06 143.51 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 99.06 148.59 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "TL1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GNDD")
		(at 39.37 87.63 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR03"
			(at 39.37 93.98 0)
		)
		(property "Value" "GND"
			(at 39.37 91.44 0)
		)
		(property "Footprint" ""
			(at 39.37 87.63 0)
		)
		(property "Datasheet" ""
			(at 39.37 87.63 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GNDD\" , digital ground"
			(at 39.37 87.63 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR03")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "lcd_display_128x64_st7920:LCD_Display_128x64_ST7920")
		(at 77.47 16.51 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U2"
			(at 119.38 52.0699 0)
		)
		(property "Value" "~"
			(at 119.38 53.975 0)
		)
		(property "Footprint" ""
			(at 77.47 16.51 0)
		)
		(property "Datasheet" ""
			(at 77.47 16.51 0)
		)
		(property "Description" ""
			(at 77.47 16.51 0)
		)
		(pin "5")
		(pin "7")
		(pin "11")
		(pin "2")
		(pin "9")
		(pin "8")
		(pin "6")
		(pin "16")
		(pin "4")
		(pin "10")
		(pin "1")
		(pin "19")
		(pin "20")
		(pin "3")
		(pin "17")
		(pin "13")
		(pin "12")
		(pin "18")
		(pin "14")
		(pin "15")
		(instances
			(project ""
				(path
					(reference "U2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GNDD")
		(at 58.42 87.63 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR02"
			(at 58.42 93.98 0)
		)
		(property "Value" "GND"
			(at 58.42 91.44 0)
		)
		(property "Footprint" ""
			(at 58.42 87.63 0)
		)
		(property "Datasheet" ""
			(at 58.42 87.63 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GNDD\" , digital ground"
			(at 58.42 87.63 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR02")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "L76K:GPS_L76K_module")
		(at 140.97 113.03 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "M1"
			(at 149.86 123.698 0)
		)
		(property "Value" "~"
			(at 167.64 126.2408 0)
		)
		(property "Footprint" ""
			(at 140.97 113.03 0)
		)
		(property "Datasheet" ""
			(at 140.97 113.03 0)
		)
		(property "Description" ""
			(at 140.97 113.03 0)
		)
		(pin "1")
		(pin "4")
		(pin "3")
		(pin "2")
		(pin "5")
		(instances
			(project ""
				(path
					(reference "M1")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
)
